#### To configure the SIP Service

1. Expand the Configuration node to select the SIP Service node.
2. In the Clusters or Enterprise profile, select the configuration you want to configure.
3. Click the SIP Service tab.
4. On the SIP Service page, you can set properties that apply to all of the service’s SIP listeners and virtual servers.

   - Enable Access Logging by virtual servers. If selected, this enables access logging for all virtual-server sub-elements that do not specify this property. If not selected, this option disables access logging for all virtual-server sub-elements that do not specify this property.

   - In the Access Log Buffer Size field, specify the size (in bytes) of the access log buffer , or a value less than or equal to zero for unbuffered access logs. The default size is 4096 bytes.

   - In the Access Log Write Interval field, specify the number of seconds before the log will be written to the disk. The access log is written when the buffer is full or when the interval expires. If the value is less than or equal to zero, then the buffer is always written even if it is not full. This means that each time the server is accessed, the log message is stored directly to the file.

5. Specify additional properties, if required.
6. Click Save.

###### See Also

- To configure the SIP Service Access Log

- To configure HTTP Service Request Processing

- To configure the HTTP Service Keep-Alive

- To configure the HTTP Service Connection Pool

- To configure the HTTP Protocol